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	1
	3D X-RAY MICROSCOPY (XRM)
	Application
Additive Manufacturing
Medical Devices and Pharmaceutical Packaging
Geology
Features
High-capacity benchtop
Latest detector technology
In-situ stages
Technical specification
X-ray source: 40-130 kV, 39 W
X-ray detector: Active pixel CMOS flat-panel, 6 MP (3072 x 1944)
Object size: 250 mm diameter, 250 mm height
Dimensions: W 1250 mm x D 815 mm x H 820 mm
Weight 450 kg
Power supply: 100-240 VAC, 50-60 Hz, 3 A max.
Documentation:
· CE marking and declaration conformity
· Documents for the Installation and Operational Qualification (IQ / OQ)
· Functional Specification - Design Qualification (DQ) and others relevant document
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